LE45 ROM FLASH TOOL GUIDE

1. Download the flash tool from our website at <https://www.lexicontech.com/le45/le45-support/> and launch the flash\_tool.exe. It is best to run the tool on Windows 10.
2. Click **choose** at **Scatter-loading File** field and browse to the ROM location as seen below. Locate and double-click the file called MT6765\_Android\_scatter.txt to load the ROM component files onto the flash tool.







1. Verify the components of the ROM image loaded on the FlashTool. Press **Download** to start loading the ROM to the device.



1. Prepare a device to connect to the PC.

Remove the battery of the device and connect the device to the PC through a USB cable. The update process will start automatically.

1. Disconnect the device once the update is completed.

